|  |  |
| --- | --- |
| **Installation Instructions**   1. Remove the 4 screws on back of the unit, using 2mm allen (hex) key. 2. Remove the back panel, unplug the power cable that connects to the front of the unit. Press the top of the connector with your finger to unlatch, pull to remove.    * If the plastic gasket comes undone with the old back panel, remove and put on the back of the unit. You can press fit with your fingers. 3. Plug the power cable from your new module to the unit. You’ll hear a click if it inserted correctly. 4. Attach your new back panel to the unit, using 4 screws. Partially tighten all screws first, then fully tight with square pattern. | **Installation Instructions**   1. Remove the 4 screws on back of the unit, using 2mm allen (hex) key. 2. Remove the back panel, unplug the power cable that connects to the front of the unit. Press the top of the connector with your finger to unlatch, pull to remove.    * If the plastic gasket comes undone with the old back panel, remove and put on the back of the unit. You can press fit with your fingers. 3. Plug the power cable from your new module to the unit. You’ll hear a click if it inserted correctly. 4. Attach your new back panel to the unit, using 4 screws. Partially tighten all screws first, then fully tight with square pattern. |
| **Installation Instructions**   1. Remove the 4 screws on back of the unit, using 2mm allen (hex) key. 2. Remove the back panel, unplug the power cable that connects to the front of the unit. Press the top of the connector with your finger to unlatch, pull to remove.    * If the plastic gasket comes undone with the old back panel, remove and put on the back of the unit. You can press fit with your fingers. 3. Plug the power cable from your new module to the unit. You’ll hear a click if it inserted correctly. 4. Attach your new back panel to the unit, using 4 screws. Partially tighten all screws first, then fully tight with square pattern. | **Installation Instructions**   1. Remove the 4 screws on back of the unit, using 2mm allen (hex) key. 2. Remove the back panel, unplug the power cable that connects to the front of the unit. Press the top of the connector with your finger to unlatch, pull to remove.    * If the plastic gasket comes undone with the old back panel, remove and put on the back of the unit. You can press fit with your fingers. 3. Plug the power cable from your new module to the unit. You’ll hear a click if it inserted correctly. 4. Attach your new back panel to the unit, using 4 screws. Partially tighten all screws first, then fully tight with square pattern. |